# FEI4B Configuration

# Module name

ModuleID		KEK122RJ1

# Geographical address

Address			1

# Global register

TrigCnt			15
Conf_AddrEnable		1
Reg2Spare		0
ErrMask0		0xffff
ErrMask1		0xffff
PrmpVbpRight		43
BufVgOpAmp		160
Reg6Spare		0
PrmpVbp			43
TdacVbp			255
DisVbn			26
Amp2Vbn			79
Amp2VbpFol		26
Reg9Spare		0
Amp2Vbp			85
FdacVbn			50
Amp2Vbpf		50
PrmpVbnFol		106
PrmpVbpLeft		43
PrmpVbpf		70
PrmpVbnLcc		0
Reg13Spare		0
PxStrobes		0
S0			0
S1			0
LVDSDrvIref		171
GADCOpAmp		100
PllIbias		88
LVDSDrvVos		105
TempSensBias		0
PllIcp			28
Reg17Spare		0
PlsrIdacRamp		213
VrefDigTune		180
PlsrVgOPamp		255
PlsrDacBias		96
VrefAnTune		0
Vthin_AltCoarse		1
Vthin_AltFine		20
PlsrDAC			45
DIGHITIN_Sel		0
DINJ_Override		0
HITLD_In		0
Reg21Spare		0
Reg22Spare2		0
Colpr_Addr		0
Colpr_Mode		0
Reg22Spare1		0
DisableColumnCnfg0	0x0
DisableColumnCnfg1	0x0
DisableColumnCnfg2	0x0
TrigLat			210
CMDcnt			11
StopModeCnfg		0
HitDiscCnfg		2
EN_PLL			1
Efuse_sense		0
Stop_Clk		0
ReadErrorReq		0
Reg27Spare1		0
GADC_Enable		0
ShiftReadBack		0
Reg27Spare2		0
GateHitOr		0
CalEn			0
SR_clr			0
Latch_en		0
SR_Clock		0
LVDSDrvSet06		1
Reg28Spare		0
EN40M			1
EN80M			0
CLK0_S2			1
CLK0_S1			0
CLK0_S0			0
CLK1_S2			0
CLK1_S1			0
CLK1_S0			0
EN160M			1
EN320M			0
Reg29Spare1		0
no8b10b			0
Clk2OutCnfg		0
EmptyRecord		0
Reg29Spare2		0
LVDSDrvEn		1
LVDSDrvSet30		1
LVDSDrvSet12		1
TempSensDiodeSel	0
TempSensDisable		0
IleakRange		0
Reg30Spare		0
PlsrRiseUpTau		7
PlsrPwr			1
PlsrDelay		2
ExtDigCalSW		0
ExtAnaCalSW		0
Reg31Spare		0
GADCSel			0
SELB0			0
SELB1			0
SELB2			0
Reg34Spare1		0
PrmpVbpMsnEn		0
Reg34Spare2		0
Chip_SN			21
Reg1Spare		0
SmallHitErase		0
Eventlimit		0

# Pixel register

enable			1
largeCap		0
smallCap		0
hitbus			0

tdac			15
fdac			7

# Charge injection parameters

cinjLo			1.891
cinjHi			3.781
vcalCoeff[0]		0.0256553
vcalCoeff[1]		0.001417
vcalCoeff[2]		0
vcalCoeff[3]		0
chargeCoeffClo		0
chargeCoeffChi		0
chargeOffsetClo		0
chargeOffsetChi		0
monleakCoeff		0